Differential Amplifier with Curr ent Pulse Generator

M2 M1

M4

MC7

Mb

M3 biasing main amplifing stage

M8 M7

M6 M5 M11

M9

M12

M10

Cc1=2.7p

First gain stage second stage

Common mode feed back cir cuit

Cc0=2.7p Iref=84uA

R2=17.7k

R1=7k

o0 o1 o0 o1 Mb1

Mb0

Mb2

Mbk Mc3 Mc4

Mc1 Mc4

Vref=2.5v

second stage

Me10

Me11

Me8 Me9 Cm1

Cm2

Non Non

Non

Pon