An Implementation of a Full y Differential Transconductance Amplifier f or a 13 Bit